{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["室温","85","Sheet3"],"not_rendered":{"comments":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"室温","index":0,"n_rows":5,"n_cols":7,"rows_kept":5,"flags":["formulas_cached_only"]}
[]
["加速因子公式","活化能","玻尔兹曼常数","常态温度","加速状态温度","常态相对湿度的n次方","加速状态相对湿度的n次方"]
["AF=exp{(Ea/k)*[(1/Tu)-(1/Ts)]+ (RHu^n-RHs^n)}","Ea(eV)","k(eV/K)","Tu(绝对温度)","Ts(绝对温度)","RHu^n(n一般取2)","RHs^n(n一般取2)"]
["AF",0.8,"8.6*10E-5",25,110,0.75,0.85]
[869.3982515024447,0.8,8.6e-05,298,383,0.5625,0.7224999999999999]

{"sheet":"85","index":1,"n_rows":11,"n_cols":7,"rows_kept":11,"flags":["formulas_cached_only"]}
[]
["加速因子公式","活化能","玻尔兹曼常数","常态温度","加速状态温度","常态相对湿度的n次方","加速状态相对湿度的n次方"]
["AF=exp{(Ea/k)*[(1/Tu)-(1/Ts)]+ (RHu^n-RHs^n)}","Ea(eV)","k(eV/K)","Tu(绝对温度)","Ts(绝对温度)","RHu^n(n一般取2)","RHs^n(n一般取2)"]
["AF",0.8,"8.6*10E-5",85,120,0.85,0.85]
[10.11591596246774,0.8,8.6e-05,358,393,0.7224999999999999,0.7224999999999999]
[]
[]
[]
[]
[1000,"试验时间","85度，85湿度"]
[{"v":98.85412291978488,"d":"99"},"试验时间","120度，85湿度"]

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}